

**Loading Soil Maps and Sample Points into SMS**


1. Import Boundary Map into SMS by going to “read files and importing from the monitor.”
2. Go to GS3 and start the automatic search, then start processing files.
3. Once you have opened the field click file, “download soil survey data from the internet (US only)”



1. Click next, select grower, farm, and field
2. Click Finish
3. Click accept if everything is correct on the screen.
4. Go into the management tree and select the field, click no year, then soil survey, no product, no instance, and select the data that named with the time and date that you imported the soil maps.



1. To add soil sample points go to file, new, soil-sampling layer.



1. Click ok with the default setting to use a wizard to create new data.
2. Select layer, click next, next
3. Select Grid Area, create sample points, click next
4. Click Finish
5. Points are uploaded onto the map.