Introduction

Now that you know how to operate a double-acting cylinder, you will operate one with DCV. The following video will explain how to set up the lab.

Lab Materials

- Directional control valve
- 3 port manifold
- FRL
- Hoses

Lab Instructions

Look at the following image and the instructions below it. The instructions will tell you how to set up the lab.

1. Make sure you are wearing safety glasses.
2. Shut off the orange shutoff valve before you start hooking up any components.
3. Plug in 2 of the 3 ports on the silver manifold.
4. Take a hose from the silver manifold and run it to the "P" port on the Manually-Operated Valve.
5. Take a 12" hose (approximate length) and run it from the "A" port on the Manually-Operated Valve to the Non-Rod side of the Double-Acting Cylinder.
6. Take a 12" hose (approximate length) and run it from the "B" port on the Manually-Operated Valve to the Rod side of the Double-Acting Cylinder.
7. Push the Manually-Operated Valve to the right.
8. Video yourself doing steps 9-11.
9. Turn on the orange shutoff valve, and set the "FR" unit to 60 psi. Check that your cylinder is retracted.
10. Shift the Manually-Operated Valve back and forth, and check that the cylinder is extending and retracting.
11. Turn off the orange shutoff valve, cycle the Manually-Operated Valve back and forth a couple of times so that there is no stored air in the system, unhook the hoses, and put everything away.

Submission

To complete this lab, submit your video according to the criteria in the rubric.

Unless specified otherwise, any and all work on this page is licensed under a Creative Commons Attribution-NonCommercial 4.0 International License.