|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |

**Capillary Action Activity**

Micropumps Learning Module

**Instructor Guide**

|  |  | |
| --- | --- | --- |
|  | Notes to Instructor | |
|  | The Capillary Action Activity is an activity for the *Micropumps Overview Learning Module*.  Following is a list of the units included in the *Micropumps Overview Learning Module*.   * Micropumps Knowledge Probe (KP) - Pretest * Micropumps Overview Primary Knowledge * Diaphragm Pump Activity * **Capillary Action Activity** * Micropumps Overview Final Assessment | |
|  | Description and Estimated Time to Complete |
|  | This activity demonstrates the capillary effect, and how liquids can flow without external input energy. You explore the limits of capillary action and the scale at which this action occurs.  Estimated Time to Complete  Allow at least 30 minutes to complete this activity. |
|  | Introduction |
|  | C:\xtProject\App_Pumps_AC11\graphics\microchannel.jpg  *Microchannel from a Piezoelectric Inkjet Printhead* |
|  | A common application of micropumps is in inkjet printing. Inkjet printheads are actually an array of micropumps used to deliver small volumes of liquid (approximately a picoliter) onto paper creating images and text. Both mechanical and non-mechanical versions of inkjet micropumps are currently in production.  One scientific phenomenon used by inkjet technology is capillary action. Bubblejet and piezoelectric inkjet printers use microchannels filled with ink. Because the microchannels' dimensions are so small (approximately a micrometer in diameter) the liquid automatically fills the microchannel due to adhesive forces between the liquid and the surfaces of the channel, and the surface tension of the liquid. |
|  | Activity Objectives and Outcomes |
|  | Activity Objectives   * Simulate the operation of an inkjet printhead by demonstrating capillary action between two narrow channels. * Explain capillary action and how it is affected by the size of the microchannel.   Activity Outcomes   * After completing this experiment, you should have a better understanding of capillary action and how this phenomenon is used in inkjet printheads. |

|  |  |
| --- | --- |
|  | Supplies |
|  | C:\Users\mj\Documents\My Dropbox\scme-scos\micropump\graphics\capillarysupplies.jpg   * Four microscope slides * Food color * Sheet of paper * Scissors * Two Pennies |
|  | Activity: Capillary Action    Procedure: |
|  | 1. From the sheet of paper, cut two ¼" x ¼" squares. 2. Place these squares of paper on two adjacent corners of a microscope slide. 3. Put the second microscope slide on top of the first, staggering it, leaving about ¼" of the bottom slide’s glass exposed. 4. Put a few drops of food coloring on of the bottom slide’s exposed glass. Observe how the food coloring moves up the slide. Let this sit while you prepare the second set of slides. 5. Using the other two microscope slides, make a similar setup using pennies instead of paper squares. 6. Put a few drops of food coloring on the bottom slide’s exposed glass. Observe how the food coloring moves up the slide. Compare the motion of the food coloring in this configuration with the previous one. 7. If you have a camera, record the results for documentation and to illustrate your responses to the Post-Activity Questions. Compare your results with those shown in this video (<https://youtu.be/vCVdSTUKwRQ> ). 8. Answer the Post-Activity Questions |

|  |  |
| --- | --- |
|  | **Notes to Instructor**  The pictures below show the results of the first set of microscope slides using the thinner spacers – the paper. The picture on the left was taken after 3 seconds of time had passed once the food coloring was placed. The two subsequent pictures were taken at 6 seconds and 15 seconds, respectively. Times will vary from one experiment to another. However, a continuous “fill” should be observed once the liquid is placed on the edge of the slides. When this experiment is repeated using the pennies, a significant change in capillary action should be observed. Have the students explain the cause and effect of what they see.    *Demonstration of Capillary Effect* |
|  | Post-Activity Questions |
|  | 1. In this activity, what is the purpose for using two different sized spacers? 2. How does the rate of flow compare between the two systems? 3. How does the flow distance compare between the two systems? 4. Write an explanation as to why the liquid behaves differently between the two systems. 5. What are three examples of capillary action (e.g., water wicking in a papertowel) |
|  | Post-Lab Questions / Answers   1. In this activity, what is the purpose for using two different sized spacers?   *To illustrate the effect that the size of the channel has on the flow of the liquid and thus the capillary action of the liquid within each channel.*   1. How does the rate of flow compare between the two systems?   *The liquid flows faster (faster flow rate) in the smaller channel. This is determined by the fact that the food coloring moved faster in the smaller spaced slides (paper spacers).*   1. How does the flow distance compare between the two systems?   *The liquid moves a farther distance in the smaller channel.*   1. Write an explanation as to why the liquid behaves differently between the two systems.   *Capillary action is strongly dependent on the distance between surfaces. The further apart the surfaces, the weaker the adhesive forces between the plates become; therefore, the narrower the channel, the stronger the interaction between the adhesive forces of the channel and the surface tension of the liquid.*   1. What are three examples of capillary action (e.g., water wicking in a papertowel)   *Ground water moving from wet areas to dry areas*  *Tears moving through tear ducts*  *Thin layer Chromatography - studying chemical separations*  *The wicking of fabrics and sponges*  *Oil lamps that use wicks* |
|  | References |
|  | * SCME Micropumps Overview Primary Knowledge Unit * Supporting video: Demonstration of Capillary Action <https://youtu.be/vCVdSTUKwRQ>   *Support for this work was provided by the National Science Foundation's Advanced Technological Education (ATE) Program. For more MEMS learning modules from SCME, please check out our website (*[*http://scme-nm.org*](http://scme-nm.org)*).* |